|  |  |  |
| --- | --- | --- |
| **RFQ/GRC/Chios-2016-007** |  |  |
| **Annex B - Term of Reference** |  |  |
| **No.** | **Item description** | **Unit** | **Quantity** | **Remarks** |  |  |
| Α. CIVIL WORKS Souda ( Installation of Fence) |   |   |   |   |  |  |
| 1 | Fencing | m | 200 | Fencing in Souda Camp. The fence panel will be rectangular 62x132mm , providing rigidity and anti-climbing features to the fence. Panels will be 25x2 mm, hot dip galvanized in reinforced by horizontal blades and vertical bars , with pillars. The height of the fence panel should be 2.5 m .The base of the fence will be footed in a movable concrete base, dimensions: length 2m to height 0,5m to width 0.2 m  |  |  |
| 2 | Construction of gate | item | 3 | Supply and construction of 3 metal gates with poles 5m wide and 3 m height. Gate should be divided into two parts a. 2.5 m & b. 1 m with all necessary fitting to lock & open as required. |  |  |
| 3 | Construction of gate | item | 2 | Supply and construction of 1 metal gates with poles 3m wide and 3 m height. Gate should be divided into two parts a. 1.5 m & b. 1 m with all necessary fitting to lock & open as required. |  |  |
| 4 | Construction of gate | item | 5 | Supply and construction of 5 metal gates with poles 1 m wide and 3 m height.  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |